**EXPERIMENT 14**

**P.N.DIODE**

**Day & Date:**

Aim: To Draw the I-V characteristics of a P.N. Diode in forward bias and hence to determine static and dynamic resistance of the diode.

Theory:

 Static resistance = Direct voltage required / Direct current required at that stage.

 Dynamic resistance = Peak to peak alternating voltage / Peak to peak alternating current

**OBSERVATIONS: CIRCUIT DIAGRAM:**

|  |  |  |
| --- | --- | --- |
| No.  | Voltmeter reading | Ammeter reading |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

RESULT:

1. Static resistance of the diode =
2. Dynamic resistance of the diode =